Back To Index << Back To Terminology

# Value Set DocumentEntry.eventCodeList 2021‑04‑01 17:00:07

From publication for project CH-EPR | Release Release 202506.1-stable as of 2026‑05‑08 11:08:13 | | | HTML built on 2026‑05‑08 11:20:16

This terminology is a snapshot as of 2026‑05‑08 11:08:13. Terminologies may evolve over time. If you need recent (dynamic) versions of this terminology, please retrieve it from the source.
Id | 2.16.756.5.30.1.127.3.10.1.8 | Effective Date | 2021‑04‑01 17:00:07 Other versions this id: DocumentEntry.eventCodeList202506.0-stable - as of 2025‑12‑01 15:45:57 DocumentEntry.eventCodeList202212.0-stable - as of 2022‑11‑29 13:34:56 DocumentEntry.eventCodeList202306.0-stable - as of 2022‑06‑26 13:44:21 DocumentEntry.eventCodeList201907.1-stable - as of 2019‑11‑03 14:33:22 DocumentEntry.eventCodeList201907.0-stable - as of 2017‑11‑15 11:33:59
Status | Deprecated | Version Label | 202104.0-stable
Name | DocumentEntry.eventCodeList | Display Name | DocumentEntry.eventCodeList
Source Code System | 1.2.840.10008.2.16.4 - DICOM Controlled Terminology - FHIR: http://dicom.nema.org/resources/ontology/DCM
Level/ Type | Code | Display Name | Code System | Designations | Description
--- | --- | --- | --- | --- | ---
0‑L | BI | Biomagnetic Imaging | DICOM Controlled Terminology | Preferred: Biomagnetic Imaging | An acquisition device, process or method that performs biomagnetic imaging.
0‑L | TG | Thermography | DICOM Controlled Terminology | Preferred: Thermography | An acquisition device, process or method that performs thermography.
0‑L | RTIMAGE | RT Image | DICOM Controlled Terminology | Preferred: RT Image | An acquisition device, process or method that performs radiotherapy imaging.
0‑L | RESP | Respiratory Waveform | DICOM Controlled Terminology | Preferred: Respiratory Waveform | A device, process or method that produces waveforms of electrical signals from the patient’s respiratory system.
0‑L | POS | Position Sensor | DICOM Controlled Terminology | Preferred: Position Sensor | An acquisition device, process or method that uses a sensor measuring the orientation or position of the patient’s body.
0‑L | PA | Photoacoustic | DICOM Controlled Terminology | Preferred: Photoacoustic | An acquisition device, process or method that performs photoacoustic imaging or acquisition.
0‑L | LS | Laser Scan | DICOM Controlled Terminology | Preferred: Laser Scan | An acquisition device, process or method that performs laser surface scanning.
0‑L | EOG | Electrooculography | DICOM Controlled Terminology | Preferred: Electrooculography | An acquisition device, process or method that performs electrooculography.
0‑L | EMG | Electromyography | DICOM Controlled Terminology | Preferred: Electromyography | An acquisition device, process or method that performs electromyography.
0‑L | EEG | Electroencephalography | DICOM Controlled Terminology | Preferred: Electroencephalography | An acquisition device, process or method that performs electroencephalography.
0‑L | DMS | Dermoscopy | DICOM Controlled Terminology | Preferred: Dermoscopy | An acquisition device, process or method that performs imaging of the surface of the skin using epiluminescence microscopy.
0‑L | DG | Diaphanography | DICOM Controlled Terminology | Preferred: Diaphanography | An acquisition device, process or method that performs diaphanography.
0‑L | CFM | Confocal Microscopy | DICOM Controlled Terminology | Preferred: Confocal Microscopy |
0‑L | OPTENF | Ophthalmic Tomography En Face | DICOM Controlled Terminology | Preferred: Ophthalmic Tomography En Face | An acquisition device, process or method that creates en face tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
0‑L | OPTBSV | Ophthalmic Tomography B-scan Volume Analysis | DICOM Controlled Terminology | Preferred: Ophthalmic Tomography B-scan Volume Analysis | An acquisition device, process or method that performs B-scan volume analysis of tomography images of the eye based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
0‑L | OPV | Ophthalmic Visual Field | DICOM Controlled Terminology | Preferred: Ophthalmic Visual Field | An acquisition device, process or method that measures visual fields and perform visual perimetry.
0‑L | DX | Digital Radiography | DICOM Controlled Terminology | Preferred: Digital Radiography | An acquisition device, process or method that performs digital radiography.
0‑L | OPT | Ophthalmic Tomography | DICOM Controlled Terminology | Preferred: Ophthalmic Tomography | An acquisition device, process or method that performs tomography of the eye that is based on light and optical principles. Tomography based on other principles, such as ultrasound, is excluded.
0‑L | BMD | Bone Mineral Densitometry | DICOM Controlled Terminology | Preferred: Bone Mineral Densitometry | An acquisition device, process or method that performs bone mineral densitometry by X-Ray, including dual-energy X-Ray absorptiometry (DXA) and morphometric X-Ray absorptiometry (MXA).
0‑L | MG | Mammography | DICOM Controlled Terminology | Preferred: Mammography | An acquisition device, process or method that performs mammography.
0‑L | SM | Slide Microscopy | DICOM Controlled Terminology | Preferred: Slide Microscopy | An acquisition device, process or method that performs slide microscopy.
0‑L | US | Ultrasound | DICOM Controlled Terminology | Preferred: Ultrasound | An acquisition device, process or method that performs ultrasound.
0‑L | OP | Ophthalmic Photography | DICOM Controlled Terminology | Preferred: Ophthalmic Photography | An acquisition device, process or method that performs ophthalmic photography.
0‑L | IVOCT | Intravascular Optical Coherence Tomography | DICOM Controlled Terminology | Preferred: Intravascular Optical Coherence Tomography | An acquisition device, process or method that performs intravascular optical coherence tomography.
0‑L | MR | Magnetic Resonance | DICOM Controlled Terminology | Preferred: Magnetic Resonance | An acquisition device, process or method that performs magnetic resonance imaging.
0‑L | ECG | Electrocardiography | DICOM Controlled Terminology | Preferred: Electrocardiography | An acquisition device, process or method that performs magnetic resonance imaging.
0‑L | GM | General Microscopy | DICOM Controlled Terminology | Preferred: General Microscopy | An acquisition device, process or method that performs electrocardiography.
0‑L | IO | Intra-oral Radiography | DICOM Controlled Terminology | Preferred: Intra-oral Radiography | An acquisition device, process or method that performs intra-oral radiography.
0‑L | XA | X-Ray Angiography | DICOM Controlled Terminology | Preferred: X-Ray Angiography | An acquisition device, process or method that performs X-Ray angiography.
0‑L | XC | External-camera Photography | DICOM Controlled Terminology | Preferred: External-camera Photography | An acquisition device, process or method that performs photography with an external camera.
0‑L | VA | Visual Acuity | DICOM Controlled Terminology | Preferred: Visual Acuity | An acquisition device, process or method that measures visual acuity.
0‑L | IVUS | Intravascular Ultrasound | DICOM Controlled Terminology | Preferred: Intravascular Ultrasound | An acquisition device, process or method that performs intravascular ultrasound.
0‑L | CR | Computed Radiography | DICOM Controlled Terminology | Preferred: Computed Radiography | An acquisition device, process or method that performs computed radiography.
0‑L | ES | Endoscopy | DICOM Controlled Terminology | Preferred: Endoscopy | An acquisition device, process or method that records images during endoscopy.
0‑L | AR | Autorefraction | DICOM Controlled Terminology | Preferred: Autorefraction | An acquisition device, process or method that measures autorefraction.
0‑L | CT | Computed Tomography | DICOM Controlled Terminology | Preferred: Computed Tomography | An acquisition device, process or method that performs computed tomography.
0‑L | OSS | Optical Surface Scanner | DICOM Controlled Terminology | Preferred: Optical Surface Scanner | An acquisition device, process or method that performs optical surface scanning.
0‑L | LEN | Lensometry | DICOM Controlled Terminology | Preferred: Lensometry | An acquisition device, process or method that performs lensometry.
0‑L | RG | Radiographic imaging | DICOM Controlled Terminology | Preferred: Radiographic imaging | An acquisition device, process or method that performs radiographic imaging (conventional film/screen).
0‑L | RF | Radiofluoroscopy | DICOM Controlled Terminology | Preferred: Radiofluoroscopy | An acquisition device, process or method that performs radiofluoroscopy.
0‑L | KER | Keratometry | DICOM Controlled Terminology | Preferred: Keratometry | An acquisition device, process or method that performs keratometry.
0‑L | HD | Hemodynamic Waveform | DICOM Controlled Terminology | Preferred: Hemodynamic Waveform | An acquisition device, process or method that records hemodynamic waveforms.
0‑L | OAM | Ophthalmic Axial Measurements | DICOM Controlled Terminology | Preferred: Ophthalmic Axial Measurements | An acquisition device, process or method that measures the axial length of the eye.
0‑L | NM | Nuclear Medicine | DICOM Controlled Terminology | Preferred: Nuclear Medicine | An acquisition device, process or method that performs nuclear medicine imaging.
0‑L | OCT | Optical Coherence Tomography | DICOM Controlled Terminology | Preferred: Optical Coherence Tomography | An acquisition device, process or method that uses an interferometric, non-invasive optical tomographic technique to image 2D slices and 3D volumes of tissue using visible and near visible frequencies.
0‑L | BDUS | Ultrasound Bone Densitometry | DICOM Controlled Terminology | Preferred: Ultrasound Bone Densitometry | An acquisition device, process or method that performs ultrasound bone densitometry.
0‑L | PT | Positron emission tomography | DICOM Controlled Terminology | Preferred: Positron emission tomography | An acquisition device, process or method that performs positron emission tomography (PET).
0‑L | EPS | Cardiac Electrophysiology | DICOM Controlled Terminology | Preferred: Cardiac Electrophysiology | An acquisition device, process or method that performs cardiac electrophysiology.
0‑L | PX | Panoramic X-Ray | DICOM Controlled Terminology | Preferred: Panoramic X-Ray | An acquisition device, process or method that performs panoramic X-Rays.
0‑L | SRF | Subjective Refraction | DICOM Controlled Terminology | Preferred: Subjective Refraction | An acquisition device, process or method that records subjective refraction.
0‑L | OPM | Ophthalmic Mapping | DICOM Controlled Terminology | Preferred: Ophthalmic Mapping | An acquisition device, process or method that measures corneal topography, corneal or retinal thickness, and other similar parameters that are typically displayed as maps.
0‑L | OPR | Ophthalmic Refraction | DICOM Controlled Terminology | Preferred: Ophthalmic Refraction | An acquisition device, process or method that measures the refractive characteristics of the eye.
Legenda: Type L=leaf, S=specializable, A=abstract, D=deprecated. NullFlavor OTH (other) suggests text in originalText. HL7 V3: NullFlavors to appear in @nullFlavor attribute instead of @code.
| XML JSON CSV SQL SVS